* **Screen firmware update log**

UI Version : 1.4

1. Fix the problem of display crash and jam.
2. Add the blue screen prompt after detecting screen error.
3. Add screen standby function: On the home screen, tap【Settings】【Advanced Settings】. Then click the brightness bar next to "Little Sun" to convert to "moon" to enable. The brightness will automatically dim after 3 minutes.
4. Fixed some known bugs.

* **Board firmware update log**

Board Firmware Version : 1.1.4

1. Add SD card read/write error warning.
2. Modify the default maximum acceleration: X1100 Y900 Z100 E1500.
3. Enable: Host Action Commands.
4. Enable: Hotbed PID, default value: M304 P97.10 I1.41 D1675.16.
5. Repair the error content of the hot end minimum temperature error displayed.

Board Firmware Version : 1.1.4.1

1. Optimize on the basis of 1.1.4.
2. Disable: Hotbed PID.
3. which will solve the problem of frequent flickering of lights in 1.1.4 firmware.
4. After the printing is done, the Y-axis may have a backward problem when pulling out the TF card (This has been optimized a little.)

Board Firmware Version : 1.1.5

1. Optimize on the basis of 1.1.4.1.
2. Enable：M303 - PID autotune.
3. Starting height of power recovery: more than 2mm.
4. Default Z Fade Height: 2mm. Reference: https://marlinfw.org/docs/gcode/M420.html
5. Support Gcode-M600 code to achieve pause.
6. Optimize the position of operation stop printing.
7. Fix some known bugs.

Board Firmware Version : 1.1.5.1

1. Improvements from 1.1.5.
2. Enable: Linear Pressure Control V1.5 ,Default value: K0.0.

**Compatibility**

|  |  |
| --- | --- |
| UI version | Board Firmware version |
| 1.4 | Neptune3Pro：1.1.4-1.1.5.1 |